# Parameters:
# instance.parameter=value       #(type, mode) default = 'def value' : description : [min..max]
#----------------------------------------------------------------------------------------------
fvp_mps2.mps2_visualisation.disable-visualisation=1   # (bool  , init-time) default = '0'      : Enable/disable visualisation
cpu0.FPU=1                                            # (bool  , init-time) default = '1'      : Set whether the model has VFP support
cpu0.DSP=1                                            # (bool  , init-time) default = '1'      : Set whether the model has the DSP extension
cpu0.semihosting-enable=1                             # (bool  , init-time) default = '1'      : Enable semihosting SVC traps. Applications that do not use semihosting must set this parameter to false.
cpu0.semihosting-Thumb_SVC=0xAB                       # (int   , init-time) default = '0xAB'   : T32 SVC number for semihosting : [0x0..0xFF]
cpu0.semihosting-cmd_line=""                          # (string, init-time) default = ''       : Command line available to semihosting SVC calls
cpu0.semihosting-heap_base=0x0                        # (int   , init-time) default = '0x0'    : Virtual address of heap base : [0x0..0xFFFFFFFF]
cpu0.semihosting-heap_limit=0x0                       # (int   , init-time) default = '0x10700000' : Virtual address of top of heap : [0x0..0xFFFFFFFF]
cpu0.semihosting-stack_base=0x0                       # (int   , init-time) default = '0x10700000' : Virtual address of base of descending stack : [0x0..0xFFFFFFFF]
cpu0.semihosting-stack_limit=0x0                      # (int   , init-time) default = '0x10800000' : Virtual address of stack limit : [0x0..0xFFFFFFFF]
cpu0.semihosting-cwd=""                               # (string, init-time) default = ''       : Base directory for semihosting file access.
cpu0.MPU_S=0x8                                        # (int   , init-time) default = '0x8'    : Number of regions in the Secure MPU. If Security Extentions are absent, this is ignored : [0x0..0x10]
cpu0.MPU_NS=0x8                                       # (int   , init-time) default = '0x8'    : Number of regions in the Non-Secure MPU. If Security Extentions are absent, this is the total number of MPU regions : [0x0..0x10]
cpu0.ITM=0                                            # (bool  , init-time) default = '1'      : Level of instrumentation trace supported. false : No ITM trace included, true: ITM trace included
cpu0.IRQLVL=0x3                                       # (int   , init-time) default = '0x3'    : Number of bits of interrupt priority : [0x3..0x8]
cpu0.BIGENDINIT=0                                     # (bool  , init-time) default = '0'      : Initialize processor to big endian mode
cpu0.INITSVTOR=0x00000000                             # (int   , init-time) default = '0x10000000' : Secure vector-table offset at reset : [0x0..0xFFFFFF80]
cpu0.INITNSVTOR=0x0                                   # (int   , init-time) default = '0x0'    : Non-Secure vector-table offset at reset : [0x0..0xFFFFFF80]
cpu0.SAU=0x8                                          # (int   , init-time) default = '0x4'    : Number of SAU regions (0 => no SAU) : [0x0..0x8]
cpu0.SAU_CTRL.ENABLE=0                                # (bool  , init-time) default = '0'      : Enable SAU at reset
cpu0.SAU_CTRL.ALLNS=0                                 # (bool  , init-time) default = '0'      : At reset, the SAU treats entire memory space as NS when the SAU is disabled if this is set
idau.NUM_IDAU_REGION=0x0                              # (int   , init-time) default = '0xA'    : 
cpu0.LOCK_SAU=0                                       # (bool  , init-time) default = '0'      : Lock down of SAU registers write
cpu0.LOCK_S_MPU=0                                     # (bool  , init-time) default = '0'      : Lock down of Secure MPU registers write
cpu0.LOCK_NS_MPU=0                                    # (bool  , init-time) default = '0'      : Lock down of Non-Secure MPU registers write
cpu0.CPIF=1                                           # (bool  , init-time) default = '1'      : Specifies whether the external coprocessor interface is included
cpu0.SECEXT=1                                         # (bool  , init-time) default = '1'      : Whether the ARMv8-M Security Extensions are included
fvp_mps2.DISABLE_GATING=1                             # (bool  , init-time) default = '0'      : Disable Memory gating logic
#----------------------------------------------------------------------------------------------
