# Parameters:
# instance.parameter=value       #(type, mode) default = 'def value' : description : [min..max]
#----------------------------------------------------------------------------------------------
fvp_mps2.mps2_visualisation.disable-visualisation=1   # (bool  , init-time) default = '0'      : Enable/disable visualisation
cpu0.semihosting-enable=1                             # (bool  , init-time) default = '1'      : Enable semihosting SVC traps. Applications that do not use semihosting must set this parameter to false.
cpu0.semihosting-Thumb_SVC=0xAB                       # (int   , init-time) default = '0xAB'   : T32 SVC number for semihosting : [0x0..0xFF]
cpu0.semihosting-cmd_line=""                          # (string, init-time) default = ''       : Command line available to semihosting SVC calls
cpu0.semihosting-heap_base=0x0                        # (int   , init-time) default = '0x0'    : Virtual address of heap base : [0x0..0xFFFFFFFF]
cpu0.semihosting-heap_limit=0x0                       # (int   , init-time) default = '0x10700000' : Virtual address of top of heap : [0x0..0xFFFFFFFF]
cpu0.semihosting-stack_base=0x0                       # (int   , init-time) default = '0x10700000' : Virtual address of base of descending stack : [0x0..0xFFFFFFFF]
cpu0.semihosting-stack_limit=0x0                      # (int   , init-time) default = '0x10800000' : Virtual address of stack limit : [0x0..0xFFFFFFFF]
cpu0.semihosting-cwd=""                               # (string, init-time) default = ''       : Base directory for semihosting file access.
idau.NUM_IDAU_REGION=0x0                              # (int   , init-time) default = '0xA'    : 
cpu0.SECEXT=0                                         # (bool  , init-time) default = '1'      : Whether the ARMv8-M Security Extensions are included
fvp_mps2.DISABLE_GATING=1                             # (bool  , init-time) default = '0'      : Disable Memory gating logic
#----------------------------------------------------------------------------------------------
